TECHNICAL DATA

CAPACITY: 			10” – 24”
MAX. RIM WIDTH:  		12”
HYDRAULIC SYS. MOT: 	0,55 Kw, 50 HZ, 380 Volt 3Ø
MAIN SHAFT MOT:  		0,18 Kw, 50 HZ, 380 Volt 3Ø
WORKING PRESSURE:  	3 preset levels ( 25-45-60 psi ) 
MAX. SYS PRESSURE:		200 psi
SOUND LEVEL:			55 db
MAX LENGTH:			500 mm.
MAX HEIGTH:			900 mm.
MAX WIDTH:			1.100 mm.
COLOR:				FERRARI ROSSO CORSA 
NET WEIGHT:			165 kg.

Electronic microprocessor to control all the machine functions and it is equipped with failures search

Electronic control cabinet on board of the machinery.

Full protection against accidents, made to ECC standards.

Warranty:		12 months after commissioning is agreed for all components.